{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["表紙","変更履歴","ピン配置","ピン配置 記入例"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":44,"defined_names":8772,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"表紙","index":0,"n_rows":39,"n_cols":4,"rows_kept":39,"cut":false,"hidden":false,"merged":[[19,3,26,32],[28,3,30,32],[38,3,43,32]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"【REA】\nCANルータ_ピン配置表"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"2025/05/28\n株式会社ハイシンク創研"]

{"sheet":"変更履歴","index":1,"n_rows":7,"n_cols":38,"rows_kept":7,"cut":false,"hidden":false,"merged":[[7,37,7,39],[8,37,8,39],[4,37,4,39],[5,37,5,39],[6,37,6,39],[20,3,20,6],[20,7,20,10],[20,12,20,32],[21,3,21,6],[21,7,21,10],[21,12,21,32],[17,3,17,6],[17,7,17,10],[17,12,17,32],[4,3,4,6],[4,7,4,10],[4,11,4,32],[5,3,5,6],[5,7,5,10],[5,12,5,32],[6,3,6,6],[6,7,6,10],[6,12,6,32],[11,3,11,6],[8,12,8,32],[9,12,9,32],[10,12,10,32],[7,3,7,6],[7,7,7,10],[7,12,7,32],[8,3,8,6],[8,7,8,10],[24,3,24,6],[24,7,24,10],[24,12,24,32],[11,7,11,10],[11,12,11,32],[13,3,13,6],[13,7,13,10],[13,12,13,32],[12,3,12,6],[12,7,12,10],[12,12,12,32],[9,3,9,6],[10,3,10,6],[9,7,9,10],[10,7,10,10],[25,3,25,6],[25,7,25,10],[25,12,25,32],[14,3,14,6],[14,7,14,10],[14,12,14,32],[18,3,18,6],[18,7,18,10],[18,12,18,32],[15,3,15,6],[15,7,15,10],[15,12,15,32],[16,3,16,6],[16,7,16,10],[16,12,16,32],[22,3,22,6],[22,7,22,10],[22,12,22,32],[23,3,23,6],[23,7,23,10],[23,12,23,32],[19,3,19,6],[19,7,19,10],[19,12,19,32],[28,3,28,6],[28,7,28,10],[28,12,28,32],[29,3,29,6],[29,7,29,10],[29,12,29,32],[26,3,26,6],[26,7,26,10],[26,12,26,32],[27,3,27,6],[27,7,27,10],[27,12,27,32],[32,3,32,6],[32,7,32,10],[32,12,32,32],[33,3,33,6],[33,7,33,10],[33,12,33,32],[30,3,30,6],[30,7,30,10],[30,12,30,32],[31,3,31,6],[31,7,31,10],[31,12,31,32],[36,3,36,6],[36,7,36,10],[36,12,36,32],[37,3,37,6],[37,7,37,10],[37,12,37,32],[34,3,34,6],[34,7,34,10],[34,12,34,32],[35,3,35,6],[35,7,35,10],[35,12,35,32],[40,3,40,6],[40,7,40,10],[40,12,40,32],[40,37,40,39],[41,3,41,6],[41,7,41,10],[41,12,41,32],[41,37,41,39],[38,3,38,6],[38,7,38,10],[38,12,38,32],[38,37,38,39],[39,3,39,6],[39,7,39,10],[39,12,39,32],[39,37,39,39],[45,7,45,10],[45,12,45,32],[45,37,45,39],[42,3,42,6],[42,7,42,10],[42,12,42,32],[42,37,42,39],[43,3,43,6],[43,7,43,10],[43,12,43,32],[43,37,43,39],[44,3,44,6],[44,7,44,10],[44,12,44,32],[44,37,44,39],[45,3,45,6],[48,3,48,6],[48,7,48,10],[48,12,48,32],[48,37,48,39],[49,3,49,6],[49,7,49,10],[49,12,49,32],[49,37,49,39],[46,3,46,6],[46,7,46,10],[46,12,46,32],[46,37,46,39],[47,3,47,6],[47,7,47,10],[47,12,47,32],[47,37,47,39],[9,37,9,39],[10,37,10,39],[11,37,11,39],[12,37,12,39],[13,37,13,39],[14,37,14,39],[19,37,19,39],[18,37,18,39],[17,37,17,39],[16,37,16,39],[15,37,15,39],[24,37,24,39],[23,37,23,39],[22,37,22,39],[21,37,21,39],[20,37,20,39],[28,37,28,39],[27,37,27,39],[26,37,26,39],[25,37,25,39],[29,37,29,39],[30,37,30,39],[31,37,31,39],[32,37,32,39],[33,37,33,39],[34,37,34,39],[35,37,35,39],[36,37,36,39],[37,37,37,39]]}
[]
[]
[null,null,"変更履歴"]
[]
[null,null,null,"バージョン",null,null,null,"更新日",null,null,null,"内容",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"担当者"]
[null,null,null,"□0-0",null,null,null,"2025-05-28",null,null,null,"・","初版"]
[null,null,null,"□0-1",null,null,null,"2025-08-29",null,null,null,"・","LED信号追加",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LHC上田"]

{"sheet":"ピン配置","index":2,"n_rows":107,"n_cols":14,"rows_kept":107,"cut":false,"hidden":false,"merged":[[5,0,5,1],[5,2,5,6],[5,7,5,11],[2,1,2,2]]}
[]
["マイコンピン配置表(R7F7016863AFP-C (RH850/F1KM-S1 100pin))",null,null,null,null,null,null,null,null,null,null,"凡例","灰色背景は用途固定端子であることを表す。"]
["ソフト名","B1 CANルータ"]
[]
[]
["素子",null,"ソフト",null,null,null,null,"ハード"]
["端子名","端子番号","端子機能","信号名","I/O","初期値","ソフト端子処理","回路図シンボル","外部端子処理","Hi論理","Lo論理","用途","備考"]
["P10_3",1]
["P10_4",2]
["P10_5",3]
["P10_15",4,"CAN1 EN","CAN1有効","O","Lo",null,"CAN1 EN",null,"無効","有効"]
["P11_0",5,"CAN0 EN","CAN0有効","O","Lo",null,"CAN0 EN",null,"無効","有効"]
["P0_0",6,"CAN0 TX","CAN0送信",null,null,null,"CAN0 TX"]
["P0_1",7,"CAN0 RX","CAN0受信",null,null,null,"CAN0 RX"]
["P0_2",8,"CAN1 RX","CAN1受信",null,null,null,"CAN1 RX"]
["P0_3",9,"CAN1 TX","CAN1送信",null,null,null,"CAN1 TX"]
["EVCC",10]
["P0_4",11,"CAN2 TX","CAN2送信",null,null,null,"CAN2 TX"]
["P0_5",12,"CAN2 RX","CAN2受信",null,null,null,"CAN2 RX"]
["P0_6",13,"CAN2 EN","CAN2有効","O","Lo",null,"CAN2 EN",null,"無効","有効"]
["P0_11",14]
["P0_12",15,"CAN5 EN","CAN5有効","O","Lo",null,"CAN5 EN",null,"無効","有効"]
["P0_13",16,"CAN5 RX","CAN5受信",null,null,null,"CAN5 RX"]
["P0_14",17,"CAN5 TX","CAN5送信",null,null,null,"CAN5 TX"]
["EVSS",18]
["P8_2",19]
["P8_10",20]
["P8_11",21]
["P8_12",22]
["JP0_5",23]
["JP0_4",24]
["JP0_3",25]
["JP0_2",26]
["JP0_1",27]
["JP0_0",28]
["RESET",29]
["EVCC",30]
["AWOVSS",31]
["AWOVCL",32]
["REGVCC",33]
["X2",34]
["X1",35]
["FLMD0",36]
["P0_10",37,"CAN4 TX","CAN4送信",null,null,null,"CAN4 TX"]
["P0_9",38,"CAN4 RX","CAN4受信",null,null,null,"CAN4 RX"]
["P0_8",39,"CAN3 TX","CAN3送信",null,null,null,"CAN3 TX"]
["P0_7",40,"CAN3 RX","CAN3受信",null,null,null,"CAN3 RX"]
["EVSS",41]
["P8_0",42,"CAN4 EN","CAN4有効","O","Lo",null,"CAN4 EN",null,"無効","有効"]
["P8_1",43,"CAN3 EN","CAN3有効","O","Lo",null,"CAN3 EN",null,"無効","有効"]
["P8_3",44,"LED_DISP","LED_DISP出力","O","Lo",null,"LED102",null,"消灯","点灯",null,null,"□0-1"]
["P8_4",45,"LED_0","LED_0出力","O","Lo",null,"LED0(LED201)",null,"消灯","点灯",null,null,"|"]
["P8_5",46,"LED_1","LED_1出力","O","Lo",null,"LED1(LED301)",null,"消灯","点灯",null,null,"|"]
["P8_6",47,"LED_2","LED_2出力","O","Lo",null,"LED2(LED401)",null,"消灯","点灯",null,null,"|"]
["P8_7",48,"LED_3","LED_3出力","O","Lo",null,"LED3(LED501)",null,"消灯","点灯",null,null,"|"]
["P8_8",49,"LED_4","LED_4出力","O","Lo",null,"LED4(LED601)",null,"消灯","点灯",null,null,"|"]
["P8_9",50,"LED_5","LED_5出力","O","Lo",null,"LED5(LED701)",null,"消灯","点灯",null,null,"|"]
["A0VSS",51]
["A0VREF",52]
["AP0_15",53]
["AP0_14",54]
["AP0_13",55]
["AP0_12",56]
["AP0_11",57]
["AP0_10",58]
["AP0_9",59]
["AP0_8",60]
["AP0_7",61]
["AP0_6",62]
["AP0_5",63]
["AP0_4",64]
["AP0_3",65]
["AP0_2",66]
["AP0_1",67]
["AP0_0",68]
["P9_0",69]
["P9_1",70]
["P9_2",71]
["P9_3",72]
["P9_4",73]
["P9_5",74]
["P9_6",75]
["EVCC",76]
["ISOVCL",77]
["ISOVSS",78]
["EVSS",79]
["P10_6",80,"DIP8","DIPスイッチ8","I","Lo",null,null,null,"-","-","予備"]
["P10_7",81,"DIP7","DIPスイッチ7","I","Lo",null,null,null,"-","-","予備"]
["P10_8",82,"DIP6","DIPスイッチ6","I","Lo",null,null,null,"-","-","予備"]
["P10_9",83,"DIP5","DIPスイッチ5","I","Lo",null,null,null,"-","-","予備"]
["P10_10",84,"DIP4","DIPスイッチ4","I","Lo",null,null,null,"-","-","予備"]
["P10_11",85,"DIP3","DIPスイッチ3","I","Lo",null,null,null,"-","-","予備"]
["P10_12",86,"DIP2","DIPスイッチ2","I","Lo",null,null,null,"-","-","予備"]
["P10_13",87]
["P10_14",88]
["P11_1",89,"DIP1","DIPスイッチ1","I","Lo",null,null,null,"-","-","予備"]
["P11_2",90]
["P11_3",91]
["P11_4",92]
["P11_5",93]
["P11_6",94]
["P11_7",95]
["EVCC",96]
["EVSS",97]
["P10_0",98]
["P10_1",99]
["P10_2",100]

{"sheet":"ピン配置 記入例","index":3,"n_rows":151,"n_cols":13,"rows_kept":151,"cut":false,"hidden":false,"merged":[[2,1,2,2],[5,0,5,1],[5,2,5,6],[5,7,5,11]]}
[]
["マイコンピン配置表(R7FA4M3AD3CFB (RA4M3 144pin))",null,null,null,null,null,null,null,null,null,null,"凡例","灰色背景は用途固定端子であることを表す。"]
["ソフト名","DTA(BDC)"]
[]
[]
["素子",null,"ソフト",null,null,null,null,"ハード"]
["端子名","端子番号","端子機能","信号名","I/O","初期値","ソフト端子処理","回路図シンボル","外部端子処理","Hi論理","Lo論理","用途","備考"]
["P400",1,"P400","-","O","L","-","-","Open","-","-","未使用処理"]
["P401",2,"P401","-","O","L","-","-","Open","-","-","未使用処理"]
["P402",3,"P402","-","O","L","-","-","Open","-","-","未使用処理"]
["P403",4,"P403","-","O","L","-","-","Open","-","-","未使用処理"]
["P404",5,"P404","-","O","L","-","-","Open","-","-","未使用処理"]
["P405",6,"P405","-","O","L","-","-","Open","-","-","未使用処理"]
["P406",7,"P406","-","O","L","-","-","Open","-","-","未使用処理"]
["P700",8,"P700","-","O","L","-","-","Open","-","-","未使用処理"]
["P701",9,"P701","-","O","L","-","-","Open","-","-","未使用処理"]
["P702",10,"P702","-","O","L","-","-","Open","-","-","未使用処理"]
["P703",11,"P703","-","O","L","-","-","Open","-","-","未使用処理"]
["P704",12,"P704","-","O","L","-","-","Open","-","-","未使用処理"]
["P705",13,"P705","-","O","L","-","-","Open","-","-","未使用処理"]
["VBATT",14,"VBATT","バッテリ電源","-","-","-","VBATT","-","-","-","-","-"]
["VCL0",15,"VCL0","LDO容量","-","-","-","VCL0","-","-","-","-","-"]
["XCIN",16,"XCIN","サブクロック入力","-","-","-","XCIN","-","-","-","-","-"]
["XCOUT",17,"XCOUT","サブクロック出力","-","-","-","XCOUT","-","-","-","-","-"]
["VSS",18,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["P213",19,"XTAL","クロック出力","-","-","-","XTAL","-","-","-","-","-"]
["P212",20,"EXTAL","クロック入力","-","-","-","EXTAL","-","-","-","-","-"]
["VCC",21,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["P713",22,"P713","-","O","L","-","-","Open","-","-","未使用処理"]
["P712",23,"P712","-","O","L","-","-","Open","-","-","未使用処理"]
["P711",24,"P711","-","O","L","-","-","Open","-","-","未使用処理"]
["P710",25,"P710","-","O","L","-","-","Open","-","-","未使用処理"]
["P709",26,"P709","-","O","L","-","-","Open","-","-","未使用処理"]
["P708",27,"P708","-","O","L","-","-","Open","-","-","未使用処理"]
["P415",28,"P415","-","O","L","-","-","Open","-","-","未使用処理"]
["P414",29,"P414","-","O","L","-","-","Open","-","-","未使用処理"]
["P413",30,"P413","-","O","L","-","-","Open","-","-","未使用処理"]
["P412",31,"P412","BDCアドレス","I",null,"-","BDC_ADD","PU","1台目","2台目","予備","増設用アドレス(T5用)"]
["P411",32,"P411","-","O","L","-","-","Open","-","-","未使用処理"]
["P410",33,"P410","-","O","L","-","-","Open","-","-","未使用処理"]
["P409",34,"P409","-","O","L","-","-","Open","-","-","未使用処理"]
["P408",35,"P408","-","O","L","-","-","Open","-","-","未使用処理"]
["P407",36,"P407","-","O","L","-","-","Open","-","-","未使用処理"]
["VSSUSB",37,"VSS_USB","USBグランド","-","-","-","VSS","-","-","-","-","-"]
["USBDM",38,"USB_DM","USBデータ-","-","-","-","D-","-","-","-","-","-"]
["USBDP",39,"USB_DP","USBデータ+","-","-","-","D+","-","-","-","-","-"]
["VCCUSB",40,"VCC_USB","USB電源","-","-","-","VCC","-","-","-","-","-"]
["P207",41,"TXD4","デバック＋生産用通信",null,null,"-","debug_RXD_BDC","PU",null,null,null,"評価ボードPmod1接続あり"]
["P206",42,"RXD4","デバック＋生産用通信",null,null,"-","debug_TXD_BDC","PU",null,null,null,"評価ボードPmod1接続あり"]
["P205",43,"P205","-","O","L","-","-","Open","-","-","未使用処理"]
["P204",44,"P204","-","O","L","-","-","Open","-","-","未使用処理"]
["P203",45,"CTX0","BDC-INV通信",null,null,"-","CAN_TX_INV","PU"]
["P202",46,"CRX0","BDC-INV通信",null,null,"-","CAN_RX_INV","PU"]
["P313",47,"P313","-","O","L","-","-","Open","-","-","未使用処理"]
["VSS",48,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["VCC",49,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["P214",50,"TCLK","TCLK","-","-","-","TCLK","-","-","-","-","デバッガ接続"]
["P211",51,"TDATA0","TDATA0","-","-","-","TDATA0","-","-","-","-","デバッガ接続"]
["P210",52,"TDATA1","TDATA1","-","-","-","TDATA1","-","-","-","-","デバッガ接続"]
["P209",53,"TDATA2","TDATA2","-","-","-","TDATA2","-","-","-","-","デバッガ接続"]
["P208",54,"TDATA3","TDATA3","-","-","-","TDATA3","-","-","-","-","デバッガ接続"]
["RES",55,"RES","リセット","-","-","-","nRESET","-","-","-","-","デバッガ接続"]
["P201",56,"MD","MD","-","-","-","MD","-","-","-","-","デバッガ接続"]
["P200",57,"NMI","マスク不可割込み","-","-","-","NMI","PD","-","-","-","NMI:使用しない"]
["P312",58,"P312","WDTクリアパルス","O","L","-","WDT_CLR"]
["P311",59,"P311","WDT抑止","O","H","-","WDT_INH"]
["P310",60,"P310","-","O","L","-","-","Open","-","-","未使用処理"]
["P309",61,"P309","-","O","L","-","-","Open","-","-","未使用処理"]
["P308",62,"P308","-","O","L","-","-","Open","-","-","未使用処理"]
["P307",63,"P307","-","O","L","-","-","Open","-","-","未使用処理"]
["P306",64,"P306","-","O","L","-","-","Open","-","-","未使用処理"]
["P305",65,"P305","-","O","L","-","-","Open","-","-","未使用処理"]
["P304",66,"P304","-","O","L","-","-","Open","-","-","未使用処理"]
["VSS",67,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["VCC",68,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["P303",69,"P303","-","O","L","-","-","Open","-","-","未使用処理"]
["P302",70,"P302","-","O","L","-","-","Open","-","-","未使用処理"]
["P301",71,"P301","-","O","L","-","-","Open","-","-","未使用処理"]
["P300",72,"TCK","テストクロック入力","-","-","-","TCK","PU","-","-","-","デバッガ接続"]
["P108",73,"TMS","テストモードセレクト","-","-","-","TMS","PU","-","-","-","デバッガ接続"]
["P109",74,"TDO","テストデータ出力","-","-","-","TDO","-","-","-","-","デバッガ接続"]
["P110",75,"TDI","テストデータ入力","-","-","-","TDI","PU","-","-","-","デバッガ接続"]
["P111",76,"P111","-","O","L","-","-","Open","-","-","未使用処理"]
["P112",77,"P112","-","O","L","-","-","Open","-","-","未使用処理"]
["P113",78,"P113","-","O","L","-","-","Open","-","-","未使用処理"]
["P114",79,"P114","-","O","L","-","-","Open","-","-","未使用処理"]
["P115",80,"P115","-","O","L","-","-","Open","-","-","未使用処理"]
["VCC",81,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["VSS",82,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["P608",83,"P608","-","O","L","-","-","Open","-","-","未使用処理"]
["P609",84,"CTX1","BAT通信",null,null,"-","CAN_TX_BAT","PU"]
["P610",85,"CRX1","BAT通信",null,null,"-","CAN_RX_BAT","PU"]
["P611",86,"P611","-","O","L","-","-","Open","-","-","未使用処理"]
["P612",87,"P612","ジャンクションボックス電源EN","O","L","-","JB_12V","PD","12V_EN","disenable"]
["P613",88,"P613","-","O","L","-","-","Open","-","-","未使用処理"]
["P614",89,"P614","-","O","L","-","-","Open","-","-","未使用処理"]
["VCC",90,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["VSS",91,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["VCL",92,"VCL","LDO容量","-","-","-","VCL","-","-","-","-","-"]
["P605",93,"P605","-","O","L","-","-","Open","-","-","未使用処理"]
["P604",94,"P604","-","O","L","-","-","Open","-","-","未使用処理"]
["P603",95,"P603","-","O","L","-","-","Open","-","-","未使用処理"]
["P602",96,"P602","-","O","L","-","-","Open","-","-","未使用処理"]
["P601",97,"P601","-","O","L","-","-","Open","-","-","未使用処理"]
["P600",98,"P600","-","O","L","-","-","Open","-","-","未使用処理"]
["VCC",99,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["VSS",100,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["P107",101,"P107","-","O","L","-","-","Open","-","-","未使用処理"]
["P106",102,"P106","-","O","L","-","-","Open","-","-","未使用処理"]
["P105",103,"GTIOC1A","双方向DD上アーム1相目","O","H","-","BDC_H1","PU","GATEOFF","GATEON",null,"24kHz"]
["P104",104,"GTIOC1B","双方向DD下アーム1相目","O","H","-","BDC_L1","PU","GATEOFF","GATEON",null,"24kHz"]
["P103",105,"GTIOC2A","双方向DD上アーム2相目","O","H","-","BDC_H2","PU","GATEOFF","GATEON",null,"24kHz"]
["P102",106,"GTIOC2B","双方向DD下アーム2相目","O","H","-","BDC_L2","PU","GATEOFF","GATEON",null,"24kHz"]
["P101",107,"P101","-","O","L","-","-","Open","-","-","未使用処理"]
["P100",108,"P100","ゲートブロック","O","H","-","BDC_GB","PU","GATEOFF","GATEON"]
["P800",109,"P800","-","O","L","-","-","Open","-","-","未使用処理"]
["P801",110,"P801","端子台温度ヒューズ(BDC)","I",null,"-","TB_FUSE_BDC","PU","異常","正常"]
["VCC",111,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["VSS",112,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["P500",113,"P500","-","O","L","-","-","Open","-","-","未使用処理"]
["P501",114,"P501","-","O","L","-","-","Open","-","-","未使用処理"]
["P502",115,"P502","-","O","L","-","-","Open","-","-","未使用処理"]
["P503",116,"P503","-","O","L","-","-","Open","-","-","未使用処理"]
["P504",117,"P504","-","O","L","-","-","Open","-","-","未使用処理"]
["P505",118,"P505","-","O","L","-","-","Open","-","-","未使用処理"]
["P506",119,"P506","-","O","L","-","-","Open","-","-","未使用処理"]
["P507",120,"P507","-","O","L","-","-","Open","-","-","未使用処理"]
["VCC",121,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["VSS",122,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["P015",123,"P015","-","O","L","-","-","Open","-","-","未使用処理"]
["P014",124,"P014","-","O","L","-","-","Open","-","-","未使用処理"]
["VREFL",125,"VREFL","ADC1基準グランド","-","-","-","VREFL","-","-","-","-","-"]
["VREFH",126,"VREFH","ADC1基準電圧","-","-","-","VREFH","-","-","-","-","-"]
["AVCC0",127,"AVCC0","アナログ電源","-","-","-","AVCC0","-","-","-","-","-"]
["AVSS0",128,"AVSS0","アナロググランド","-","-","-","AVSS0","-","-","-","-","-"]
["VREFL0",129,"VREFL0","ADC0基準グランド","-","-","-","VREFL0","-","-","-","-","-"]
["VREFH0",130,"VREFH0","ADC0基準電圧","-","-","-","VREFH0","-","-","-","-","-"]
["P009",131,"P009","-","O","L","-","-","Open","-","-","未使用処理"]
["P008",132,"P008","-","O","L","-","-","PD","-","-","未使用処理"]
["P007",133,"P007","-","O","L","-","-","Open","-","-","未使用処理"]
["P006",134,"P006","-","O","L","-","-","Open","-","-","未使用処理"]
["P005",135,"AN005","12V 検出","A","-","-","12V_DET"]
["P004",136,"AN004","CPU温度(雰囲気温度)","A","-","-","CPU_TMP"]
["P003",137,"AN003","パワーデバイス温度検出","A","-","-","IGBT_TEMP"]
["P002",138,"AN002","電池出力電圧(中間DC電圧)","A","-","-","BUS_BDC",null,null,null,null,"0ch/1chどちらも対応できる"]
["P001",139,"AN001","電池入力電流","A","-","-","BDC_I",null,null,null,null,"0ch/1chどちらも対応できる"]
["P000",140,"AN000","電池入力電圧","A","-","-","BDC_V",null,null,null,null,"0ch/1chどちらも対応できる"]
["VSS",141,"VSS","マイコングランド","-","-","-","VSS","-","-","-","-","-"]
["VCC",142,"VCC","マイコン電源","-","-","-","VCC","-","-","-","-","-"]
["P512",143,"P512","-","O","L","-","-","Open","-","-","未使用処理"]
["P511",144,"P511","-","O","L","-","-","Open","-","-","未使用処理"]